These are some ways to advance CCELD.

The technique itself

1. Use reverse weights in getting average. Currently CCELD uses average of neighbouring pixels but what if further pixels have higher weights and then we also still subtract from center pixel.
2. Local thresholding or say adaptive thresholding on subtracted image. Maybe I could try that directly with the adaptive thresholding function in Opencv.

The app